# DCPad

class aluvia.all.DCPad(*args, **kwargs)

  A metal pad that can be interconnected to the metal lines and contacted through a probe or through wire-bonding.

  Parameters:
    name: String that contains only ISO/IEC 8859-1 (extended ASCII py3) or pure ASCII (py2) characters

      The unique name of the pcell

  Views

  class Layout(*args, **kwargs)
    Parameters:
      length: float and number > 0

        Pad Length [um]

      width: float and number > 0

        Pad Width [um]

  Name | Type | Position | Angle | Waveguide Template | Inclination
  --- | --- | --- | --- | --- | ---
  dc0 | Electrical | (0.0, 0.0) | 0.0 | MetalWireTemplate | 0.0

      from aluvia import technology
      from aluvia.all import DCPad

      lo = DCPad().Layout()
      lo.visualize(annotate=True)