# DCPadArray

class aluvia.all.DCPadArray(*args, **kwargs)

  Array of DCPad.

  Parameters:
    name: String that contains only ISO/IEC 8859-1 (extended ASCII py3) or pure ASCII (py2) characters

      The unique name of the pcell

  Views

  class Layout(*args, **kwargs)
    Parameters:
      n_o_pads: tuple2 and Tuple of <class ‘int’> and length == 2

        number of DCPads in x and y

      pad_length: float and number > 0

        Pad Length [um]

      pad_width: float and number > 0

        Pad Width [um]

      pitch: float and number > 0

        Pitch of the DCPads [um]

  Name | Type | Position | Angle | Waveguide Template | Inclination
  --- | --- | --- | --- | --- | ---
  dc0 | Electrical | (0.0, -500.0) | 0.0 | MetalWireTemplate | 0.0
  dc1 | Electrical | (0.0, 0.0) | 0.0 | MetalWireTemplate | 0.0
  dc2 | Electrical | (0.0, 500.0) | 0.0 | MetalWireTemplate | 0.0

      from aluvia import technology
      from aluvia.all import DCPadArray

      lo = DCPadArray().Layout()
      lo.visualize(annotate=True)