# StripWaveguide_369

class aluvia.all.StripWaveguide_369(*args, **kwargs)

  Strip Waveguide operating at 369nm wavelength.

  Parameters:
    name: String that contains only ISO/IEC 8859-1 (extended ASCII py3) or pure ASCII (py2) characters

      The unique name of the pcell

  Views

  class Layout(*args, **kwargs)
    Parameters:
      shape: Shape

        Shape from which the Trace is calculated

      bend_radius: float and number > 0

        Bend radius for the auto-generated bends.

  Name | Type | Position | Angle | Waveguide Template | Inclination
  --- | --- | --- | --- | --- | ---
  in0 | Optical | (0.0, 0.0) | 180.0 | WG_TMPL | 0.0
  out0 | Optical | (100.0, 0.0) | 0.0 | WG_TMPL | 0.0

      from aluvia import technology
      from aluvia.all import StripWaveguide_369

      lo = StripWaveguide_369().Layout()
      lo.visualize(annotate=True)